CAPACITY

Auto 1oom/ power loom production capacity of 1 lakh meters/month.

FABRIC PRODUCTION LEAD TIME

i• Desk loom in 5 days

••• Production sample in 15 days for power loom, 30 days for Auto loom from approval

•'• Bulk dispatch starts from 30" day onwards

* Ordcr completion TO-55 days (According to quantity)

I ooin Tie- ups - 60 Rapier GTX and Gamma looms Fabric width - 55” to 64”

DYEING PROCESS

1. Dycing only in cone (checse) & cabinet (hanks)
2. Using brandcd dyes that is 100% AZO free. DYEING STAND.ORDS

l. Rubbing

Wet 3-4

Dry 4-5

". Shadc change - 4

3 Staining on cotton - 4

FINISHIV G PROCESS

